;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
; This file contains some register settings that are necessary to
; adjust certain register values in the VFG frame grabber in order
; to make it work with the I2S camera
; Specify one register offset and one register value per line.
; Values are hexadecimal; they have to begin with a digit.
; Note that only register offsets have to be specified: the register
; base address is found in the installation database.
;
1ch   0dfe4    ;zoom register, regmux = 01 to select variable scan register
1ah   0ff18    ;variable scan: dig. in, act.high line & field en., non-interlaced
