;                   TIM Image Specification File
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
; This file specifies the image set-up for TIMWIN.
; The specification consists of the following fields, which are separated
; by white space characters (i.e. spaces or tabs).
;
;  i  dis  8  512  512   0   0 
;  ^   ^   ^   ^    ^    ^   ^ 
;  |   |   |   |    |    +---+------position of upper left corner in field
;  |   |   |   |    |               (specify for child images only)
;  |   |   |   +----+---------------image size (Y, X)
;  |   |   +------------------------pixel size
;  |   +----------------------------type of image store: dis(play), mem(ory),
;  |                                win (memory image with Windows display)
;  +--------------------------------image name (may be any string)
;
; Images can share the same memory space if they are specified in a single
; block. An empty line separates blocks.
;
; The first line in a block not only specifies an image, but also the total
; amount of memory of the block. This first image is called: Master Image (MI).
; The image specifications following the MI may have a '-' in the image store
; type field. These images are called: child images. Their size and position
; must be so, that they fit in the master image completely. The position
; specification is necessary only with child images.
; Windows images (type 'win') cannot have children.
; Image specification blocks must be separated by at least one empty line.
;
; For every specified image the following sub-images are recognized:
; - 4 images occupying 1/4 of the total image space, accessible by appending
;   a number (1 - 4) to the image name (e.g. a1, p2, etc.).
; - a variable sub image, accessible by appending a 'c' to the image name
;   (e.g. 'ac').
;
; The first non-comment line specifies the display window: this is the size
; of the area that the frame grabber shows in non-zoomed condition.
;
; In this file coordinates are specified in Y, X fashion.
;
; In this file characters between the comment character (;) and end-of-line
; are ignored.
; ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;             Specification for 512x512 Cortex1 Frame Grabber
;
; Since this FG has only 1 display page, some image names have been relocated
; to memory. This keeps the system compatible for applications, written for
; other frame grabbers.

display = 512 512                       ;Size display window

fg  dis  8  512   512                   ;master image (determined by display)
x    -   -  512   512     0    0
p    -   -  256   256     0    0
q    -   -  256   256     0  256
r    -   -  256   256   256    0
s    -   -  256   256   256  256


;
;  Additional storage in computer memory
;
f  mem  64  256   256                   ;fft image (64-bit pixels): 512KB
e16 -   16  512   512     0     0 
m16 -   16  256   256     0     0
e   -    8  512   512     0     0
y   -    8  512   512     0   512       ;y is usually located in the frame grabber
g   -    8  512   512     0   512       ;image for graphics (as y)
a   -    8  256   256     0     0
b   -    8  256   256     0   256
c   -    8  256   256   256     0
d   -    8  256   256   256   256
t   -    8  256   256     0  1024       ;t,u,v & w are usually located in the FG
u   -    8  256   256     0  1280
v   -    8  256   256     0  1536
w   -    8  256   256     0  1792

h  win   8  256   256    

i  win   8  256   256
