;                   TIM Image Specification File
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
; This file specifies the image set-up for TIMWIN. It must be renamed
; to 'images.tim' and placed in the TIMWIN directory to become valid.
; The specification consists of the following fields, which are separated
; by white space characters (i.e. spaces or tabs).
;
;  i  dis  8  512  512   0   0 
;  ^   ^   ^   ^    ^    ^   ^ 
;  |   |   |   |    |    +---+------position of upper left corner in field
;  |   |   |   |    |               (specify for child images only)
;  |   |   |   +----+---------------image size (Y, X)
;  |   |   +------------------------pixel size
;  |   +----------------------------type of image store: dis(play), mem(ory),
;  |                                win (memory image with Windows display)
;  +--------------------------------image name (may be any string)
;
; Images can share the same memory space if they are specified in a single
; block. An empty line separates blocks.
;
; The first line in a block not only specifies an image, but also the total
; amount of memory of the block. This first image is called: Master Image (MI).
; The image specifications following the MI may have a '-' in the image store
; type field. These images are called: child images. Their size and position
; must be so, that they fit in the master image completely. The position
; specification is necessary only with child images.
; Windows images (type 'win') cannot have children.
; Image specification blocks must be separated by at least one empty line.
;
; For every specified image the following sub-images are recognized:
; - 4 images occupying 1/4 of the total image space, accessible by appending
;   a number (1 - 4) to the image name (e.g. a1, p2, etc.).
; - a variable sub image, accessible by appending a 'c' to the image name
;   (e.g. 'ac').
;
; The first non-comment line specifies the display window: this is the size
; of the area that the frame grabber shows in non-zoomed condition.
;
; In this file coordinates are specified in Y, X fashion.
;
; In this file characters between the comment character (;) and end-of-line
; are ignored.
; ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
;           Specification for 512x512 ITI-PCVision Frame Grabber
; Since this FG has only 1 display page, some image names have been relocated
; to memory. This keeps the system compatible.

display = 512 512                       ;Size display window

fg  dis    8   512   512                ;master image (determined by display)
x    -     -   512   512     0     0
p    -     -   256   256     0     0
q    -     -   256   256     0   256
r    -     -   256   256   256     0
s    -     -   256   256   256   256


;
;  Additional storage in computer memory
;
f   mem   64   256   256                ;fft image (64-bit pixels): 512KB
e16  -    16   512   512     0     0 
m16  -    16   256   256     0     0
e    -     8   512   512     0     0
y    -     8   512   512     0   512    ;y is usually located in the frame grabber
g    -     8   512   512     0  1024    ;image for graphics (as y)
a    -     8   256   256     0     0
b    -     8   256   256     0   256
c    -     8   256   256   256     0
d    -     8   256   256   256   256
t    -     8   256   256     0  1024    ;t,u,v & w are usually located in the FG
u    -     8   256   256     0  1280
v    -     8   256   256     0  1536
w    -     8   256   256     0  1792
          
h   win    8   256   256    
              
i   win    8   256   256
