            TrueTTY radioteletype software v1.30

   Program to receive and transmit RTTY and PSK31 (BPSK mode) via sound card.
No additional hardware required - you need only transceiver and computer with
sound card. Optionally you can use  simple circuit for PTT-control. It make
fast and convenient frequence control, has a lot macros for tramsmitting. Can
cooperate with RZ4AG AAlog logger.

   Shareware ($35).

   Run setup.exe to install.

   The program is freely distributable, but you must distribute the original
archive unmodified.

Sergei Podstrigailo,
UA9OSV

http://www.dxsoft.com
mailto:amx@dxsoft.com


