Windows NT Installation Intructions for the HP ScanJet IIcx SCSI 
interface (C2502-66500 and C2503-66500)


Scanner Support
===============
This installation process supports the HP ScanJet IIcx, IIp, and IIc 
scanners connected to the HP ScanJet IIcx SCSI interface card (C2502-
66500 for ISA, or C2053-66500 for Microchannel). The HP ScanJet, ScanJet 
Plus scanners, and the HP ScanJet IIc and IIp scanners connected to the 
HP ScanJet II interface card (C1752-66500 or C1753-66500) are not 
supported.


Manually installing the Windows NT drivers for the HP ScanJet IIcx SCSI 
interface card (C2502-66500 and C2503-66500)
=======================================================================
The installation instructions assume you installed Windows NT using the 
default directory settings. If you did not use the default directory 
settings, substitute the drive and path you specified for installing 
Windows NT for the C:\WINNT in the following instructions.

1. Copy the following files into the following directories:

               FILE                         Directory
               ----                         ---------
     A:\NT\DESKSCAN\HPSCAN16.SYS     C:\WINNT\SYSTEM32\DRIVERS
     A:\NT\DESKSCAN\HPSCAN32.DLL     C:\WINNT\SYSTEM32

2. Use Note Pad to add the following line to the end of the CONFIG.NT 
   file in the C:\WINNT\SYSTEM32 directory:

     device=%systemroot%\system32\drivers\HPSCAN16.SYS

3. Double Click the Main program group in the Program Manager

4. Double Click the Windows NT Setup icon.

5. The WINDOWS NT SETUP dialog box appears. Select Add/Remove SCSI 
   Adapters from the Options menu.

6. The SCSI ADAPTER SETUP dialog box appears. Click the Add button.

7. The SELECT SCSI ADAPTER OPTION dialog box appears. Scroll down and 
   select Other in the Adapter combo-box.

8. The INSERT DISKETTE dialog box appears. Insert the disk with the HP 
   SCSI drivers into drive A:. Overwrite the drive path with 
   A:\NT\NCR and click OK.

9. The SELECT OEM OPTION dialog box appears. Select the NCR SDMS 53C400A 
   SCSI driver -- HP400NT - 3.00.02 and click OK.

10. You will return to the SELECT SCSI ADAPTER OPTION dialog box. Select 
    the NCR SDMS 53C400A -- HP400NT - 3.00.02 option and click Install.

11. The WINDOWS NT SETUP dialog box appears -- asking for the full path 
    to the OEM SCSI adapter files (A:\). Click Continue.

12. You will return to the SCSI ADAPTER SETUP dialog box. Click Close.

13. You will return to the WINDOWS NT SETUP dialog box. Select Exit from 
    the Option menu.

14. Select Run from the Program Manager File menu.

15. Type REGEDT32 and click OK.

16. The Regedt32 window appears. Select the HKEY_LOCAL_MACHINE window.

17. Double-click on SYSTEM

18. Double-click on CurrentControlSet

19. Double-click on Services

20. Double-click on Scsiscan

21. SINGLE-click on Start:REG_DWORD

22. Select DWORD from the Edit menu.

23. Specify 0 in the Data field and click OK.

24. Close REGEDT32

25. Shut down Windows NT.
