
NOTES ON NEW FEATURES ADDED FOR HUBBLE 1.20 and latter
      HUBBLE ver. 1.20 and latter add another mode of operation, 
      namely [DOCUMENT BASED PROCESSING], in addition to 
      original [IMAGE BASED PROCESSING] mode. 
      With [DOCUMENT BASED PROCESSING] mode, users can
      also do desktop publishing without exiting from HUBBLE.
      Switch to [DOCUMENT BASED PROCESSING] mode from 
      [Option Menu], then load a sample HUBBLE document file
      *HUBBLE.PUB* to practice on how to use this new mode.
      For detail, see HUBBLE online help. Files *NEWINFO.TXT* 
      and *TUTORIAL.TXT" contain some info and tutorial.

NOTES ON INSTALLATION

      A. TO INSTALL FROM HARDDISK

         1. Copy every files to a harddisk directory, e.g. C:\TEMP
            
         2. Decompress HUBBLE.ZIP (pkunzip hubble)
            (If it expand to two ZIP files, HUBBLE1.ZIP and HUBBLE2.ZIP,
             Then decompress  HUBBLE1.ZIP and HUBBLE2.ZIP using
            
            pkunzip hubble?  OR pkunzip *
            
         3. Install the program.
            3.1 From Windows program manager, open file menu (Alt+F)
                and choose "RUN".
            3.2 Type C:\TEMP\INSTALL [-s] and follow the instruction.


      B. TO INSTALL FROM FLOPPY DISK (MAKE FLOOPY INSTALLATION DISKETTES)

         B1. If your copy of HUBBLE come with two distribution diskettes.

             1. Insert diskette number 1 in drive A: (or B:)
             2. From Windows program manager, open file menu (Alt+F)
                and choose "RUN"
             3. Type A:\INSTALL (or B:\INSTALL) and follow the instruction.
       
         B2. If your copy of HUBBLE is obtained from BBS or shareware vendor,
             it will consists of one or two ZIP compressed files (HUBBLE?.ZIP) 
             1. Build installation diskettes from 2 ZIP files
                1.1 Decompress HUBBLE.ZIP which should be expanded to 
                    HUBBLE1.ZIP and HUBBLE2.ZIP (pkunzip hubble)
            
                1.2. Decompress (Expand) HUBBLE1.ZIP to a temporary directory
                     (pkunzip hubble1), then copy all (decompressed) files to 
                     a high density diskette and label it as
                     Disk # 1:Install and Program Disk.

                1.3. Decompress (Expand) HUBBLE2.ZIP to a temporary directory
                     (pkunzip hubble2),  then copy all (decompressed) files to 
                     a high density diskette and label it as
                     Disk # 2:Samples and Data Disk

             2. Build installation diskettes from one ZIP file.
                2.1 Decompress HUBBLE.ZIP on a harddisk directory
                2.2 Run "TOFLOPPY A" or "TOFLOPPY B"

             3. Install HUBBLE as outlined in B1

      C. PROBLEM WITH INSTALLATION
         If for any reason you can't install HUBBLE, such as some installation
         files are corrupted, etc. Then follow the following steps:
         1. Create an empty subdirectory, such as C:\HUBBLE and go to that 
            subdirectory. e.g. 
            C:         <Enter>
            CD \       <Enter>            
            MD HUBBLE  <Enter>
            CD HUBBLE  <Enter>
         2. Unpack (UnZIP) every file to HUBBLE subdirectory, e.g.
            pkunzip d:\path\hubble?  OR pkunzip d:\path\*
         3. Expand hubble.ex_ ==> hubble.exe using "Expand" program
            come with Windows 3.x
            expand -r hubble.ex_ .
         4. If you also want to acquire image using TWAIN compatible
            scanners/devices, copy the following files:
            *** please check files contents before copying ***
            4.1 all DLL files *.DLL to Windows and System subdirectory.
                e.g. C:\WINDOWS and C:\WINDOWS\SYSTEM
            4.2 All *.ds files to TWAIN subdirectory of the Windows directory,
                e.g. C:\WINDOWS\TWAIN. You may have to go to C:\WINDOWS to
                create TWAIN subdirectory.
            4.3 You may have to contact your Scanners/Devices manufacturer to
                get the latest driver for TWAIN compatible devices.

NOTES ON CORRUPTED FILES OR DEFECTIVE DISKETTES

      If for any reason, any of your HUBBLE files is corrupted or 
      diskette received is defective, please contact HUBBLE SOFTWARE COMPANY 

      1. VIA COMPUSERVE MAIL:
         Compuserve ID to contact HUBBLE SOFTWARE COMPANY is 74544,3676      
      2. BY MAIL:
              HUBBLE SOFTWARE COMPANY             
              P.O. Box 1654                       
              Denton, TX 76202                    
              U.S.A.                              

      
NOTES: To install HUBBLE on OS/2
       a.) If HUBBLE is already installed on Windows:
           At OS/2 command prompt, type MIGRATE and follow 
           the instruction to migrate HUBBLE to OS/2.
       b.) If HUBBLE is NOT already installed on Windows:
           (OS/2 is the only system)
           Run FULL SCREEN WINDOWS from OS/2, and install HUBBLE
           as you would install on Windows. After that, at OS/2 
           command prompt, type MIGRATE and follow the instruction 
           to migrate HUBBLE to OS/2 desktop.

