;                   TIM Image Specification File
;~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
; This file specifies the image set-up for TIMWIN. It must be renamed
; to 'images.tim' and placed in the TIMWIN directory to become valid.
; The specification consists of the following fields, which are separated
; by white space characters (i.e. spaces or tabs).
;
;  i  dis  8  512  512   0   0 
;  ^   ^   ^   ^    ^    ^   ^ 
;  |   |   |   |    |    +---+------position of upper left corner in field
;  |   |   |   |    |               (specify for child images only)
;  |   |   |   +----+---------------image size (Y, X)
;  |   |   +------------------------pixel size
;  |   +----------------------------type of image store: dis(play), mem(ory),
;  |                                win (memory image with Windows display)
;  +--------------------------------image name (may be any string)
;
; Images can share the same memory space if they are specified in a single
; block. An empty line separates blocks.
;
; The first line in a block not only specifies an image, but also the total
; amount of memory of the block. This first image is called: Master Image (MI).
; The image specifications following the MI may have a '-' in the image store
; type field. These images are called: child images. Their size and position
; must be so, that they fit in the master image completely. The position
; specification is necessary only with child images.
; Windows images (type 'win') cannot have children.
; Image specification blocks must be separated by at least one empty line.
;
; For every specified image the following sub-images are recognized:
; - 4 images occupying 1/4 of the total image space, accessible by appending
;   a number (1 - 4) to the image name (e.g. a1, p2, etc.).
; - a variable sub image, accessible by appending a 'c' to the image name
;   (e.g. 'ac').
;
; The first non-comment line specifies the display window: this is the size
; of the area that the frame grabber shows in non-zoomed condition.
;
; In this file coordinates are specified in Y, X fashion.
;
; In this file characters between the comment character (;) and end-of-line
; are ignored.
;
; ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
; In this file memory occupation is minimized for use in systems with
; limited memory (e.g. 2MB)

;           Specification for 1024x1024 ITI-VFG frame grabber

display = 512 768                       ;Size display window

fg  dis  12 1024  1024                  ;master image (determined by display)
m    -    -  512   768     0     0      ;display size images
n    -    -  512   768   512     0
x    -    -  512   512     0     0      ;512x512 images
y    -    -  512   512     0   512
z    -    -  512   512   512     0
g    -    -  512   512   512   512      ;image for graphics
p    -    -  256   256     0     0      ;256x256 images
q    -    -  256   256     0   256
r    -    -  256   256   256     0
s    -    -  256   256   256   256
t    -    -  256   256     0   512
u    -    -  256   256     0   768
v    -    -  256   256   256   512
w    -    -  256   256   256   768


;
;  Additional storage in computer memory
;
m16 mem  16  256   256    
a    -    8  256   256     0     0
b    -    8  256   256   256     0

h   win   8  256   256                     ;64KB

i   win   8  256   256                     ;64KB
